|  |  |  |  |
| --- | --- | --- | --- |
| Description | [Command] | [Parameter1] | [Parameter2] |
| Auto Capture Using Sonar | 01 | 00/01  00: Turned off  01: Turned on | xx |
| Manual Capture | 02 | 00/01  00: No recognition  01: Recognize | xx |
| Minimum Auto Capture Range | 03 | Minimum  20 < min < 40  value = 00: unchanged  value = 99: default loaded | Maximum  20 < max < 60  **P.S. Max > Min** |

All the numbers are unsigned decimals (not hexadecimals)

Example string message: 010010

Each packet is 6 bytes long and broken into 2 bytes chunks for each part.

Example mosquito control command:

*mosquitto\_pub -h 142.93.62.203 -t Control -m 010010*